# XFree86[tm] Manual pages: Section 4

- XF86Config - Configuration File for XFree86
- apm - Alliance ProMotion video driver
- chips - Chips and Technologies video driver
- cirrus - Cirrus Logic video driver
- citron - Citron Infrared Touch Driver (CiTouch)
- cyrix - Cyrix video driver
- dmc - DMC input driver
- dynapro - Dynapro input driver
- elographics - Elographics input driver
- fbdev - video driver for framebuffer device
- fbdevhw - os-specific submodule for framebuffer device access
- geode - Geode video driver
- glint - GLINT/Permedia video driver
- i128 - Number 9 I128 video driver
- i740 - Intel i740 video driver
- i810 - Intel i810 video driver
- imstt - Integrated Micro Solutions Twin Turbo 128 driver
- js_x - JamStudio input driver
- kbd - Keyboard input driver
- keyboard - Keyboard input driver
- mga - Matrox video driver
- microtouch - MicroTouch input driver
- mouse - Mouse input driver
- mutouch - Microtouch input driver
- neomagic - Neomagic video driver
- newport - Newport video driver
- nv - NVIDIA video driver
- penmount - PenMount input driver
- r128 - ATI Rage 128 video driver
- rendition - Rendition video driver
- s3virge - S3 ViRGE video driver
- savage - S3 Savage video driver
- siliconmotion - Silicon Motion video driver
- sis - SiS video driver
- tdfx - 3Dfx video driver
- tek4957 - Tektronix 4957 input driver
- trident - Trident video driver
- tseng - Tseng Labs video driver
- vesa - Generic VESA video driver
- vga - Generic VGA video driver
- vmware - VMware SVGA video driver
- void - null input driver
- wacom - Wacom input driver