Table of Contents

## Name

i810 - Intel 8xx integrated graphics chipsets

## Synopsis

    Section "Device"
      Identifier "devname"
      Driver "i810"
      ...
    EndSection

## Description

i810 is an XFree86 driver for Intel integrated graphics chipsets. The driver supports depths 8, 15, 16 and 24. All visual types are supported in depth 8, other depths only support TrueColor. The driver supports hardware accelerated 3D via the Direct Rendering Infrastructure (DRI), but only in depth 16 for the i810/i815 and depths 16 and 24 for later chipsets.

## Supported Hardware

i810 supports the i810, i810-DC100, i810e, i815, 830M, 845G, 852GM, 855GM, and 865G chipsets.

## Configuration Details

Please refer to XF86Config(4) for general configuration details. This section only covers configuration details specific to this driver.

The Intel 8xx family of integrated graphics chipsets has a unified memory architecture and uses system memory for video ram. By default 8 Megabytes of system memory are used for graphics. For the 830M and later, the default is 8 Megabytes when DRI is not enabled and 32 Megabytes with DRI is enabled. This amount may be changed with the VideoRam entry in the config file Device section. It may be set to any reasonable value up to 64MB for older chipsets or 128MB for newer chipets. Note that increasing this value will reduce the amount of system memory available for other applications.

The following driver Options are supported

Option "NoAccel" "boolean"
  Disable or enable acceleration. Default: acceleration is enabled.
Option "SWCursor" "boolean"
  Disable or enable software cursor. Default: software cursor is disable and a hardware cursor is used.
Option "ColorKey" "integer"
  This sets the default pixel value for the YUV video overlay key. Default: undefined.
Option "CacheLines" "integer"
  This allows the user to change the amount of graphics memory used for 2D acceleration and video. Decreasing this amount leaves more for 3D textures. Increasing it can improve 2D performance at the expense of 3D performance. Default: 256 to 768 depending on the resolution and depth.

## See Also

XFree86(1) , XF86Config(4) , xf86config(1) , Xserver(1) , X(7)

## Authors

Authors include: Keith Whitwell, and also Jonathan Bian, Matthew J Sottek, Jeff Hartmann, Mark Vojkovich, Alan Hourihane, H. J. Lu. 830M and 845G support reworked for XFree86 4.3 by David Dawes and Keith Whitwell. 852GM, 855GM, and 865G support added by David Dawes and Keith Whitwell.

Table of Contents

- Name
- Synopsis
- Description
- Supported Hardware
- Configuration Details
- See Also
- Authors