Table of Contents

## Name

ucs2any - generate BDF fonts containing subsets of ISO 10646-1 codepoints

## Synopsis

ucs2any [ +d | -d ] source-name { mapping-file registry-encoding } ...

## Description

ucs2any allows one to generate from an ISO 10646-1 encoded BDF font other BDF fonts in any possible encoding. This way, one can derive from a single ISO 10646-1 master font a whole set of 8-bit fonts in all ISO 8859 and various other encodings.

## Options

+d
  puts DEC VT100 graphics characters in the C0 range (default for upright, character-cell fonts).
-d
  omits DEC VT100 graphics characters from the C0 range (default for all font types except upright, character-cell fonts).

## Operands

source-name
  is the name of an ISO 10646-1 encoded BDF file.
mapping-file
  is the name of a character set table like those at <ftp://ftp.unicode.org/Public/MAPPINGS/>. These files can also typically be found installed in the /usr/X11R6/lib/X11/fonts/util/ directory.
registry-encoding
  are the CHARSET_REGISTRY and CHARSET_ENCODING field values for the font name (XLFD) of the target font, separated by a hyphen.

Any number of mapping-file and registry-encoding operand pairs may be specified.

## Example

The command

> ucs2any 6x13.bdf 8859-1.TXT iso8859-1 8859-2.TXT iso8859-2

will generate the files 6x13-iso8859-1.bdf and 6x13-iso8859-2.bdf.

## Future Directions

Hopefully a future XFree86 release will have a facility similar to ucs2any built into the server, and reencode ISO 10646-1 on the fly, because storing the same fonts in many different encodings is clearly a waste of storage capacity.

## See Also

bdftruncate(1)

## Author

ucs2any was written by Markus Kuhn.

Branden Robinson wrote this manual page, originally for the Debian Project.

Table of Contents

- Name
- Synopsis
- Description
- Options
- Operands
- Example
- Future Directions
- See Also
- Author