Table of Contents

## Name

gluNextContour - mark the beginning of another contour

## C Specification

void gluNextContour( GLUtesselator* tess,

        GLenum type )

eqn not supported

## Parameters

tess
  Specifies the tessellation object (created with gluNewTess).
type
  Specifies the type of the contour being defined. Valid values are GLU_EXTERIOR, GLU_INTERIOR, GLU_UNKNOWN, GLU_CCW, and GLU_CW.

## Description

gluNextContour is used in describing polygons with multiple contours. After the first contour has been described through a series of gluTessVertex calls, a gluNextContour call indicates that the previous contour is complete and that the next contour is about to begin. Another series of gluTessVertex calls is then used to describe the new contour. This process can be repeated until all contours have been described.

type defines what type of contour follows. The legal contour types are as follows:

GLU_EXTERIOR
  An exterior contour defines an exterior boundary of the polygon.
GLU_INTERIOR
  An interior contour defines an interior boundary of the polygon (such as a hole).
GLU_UNKNOWN
  An unknown contour is analyzed by the library to determine if it is interior or exterior.
GLU_CCW,
GLU_CW
  The first GLU_CCW or GLU_CW contour defined is considered to be exterior. All other contours are considered to be exterior if they are oriented in the same direction (clockwise or counterclockwise) as the first contour, and interior if they are not.

If one contour is of type GLU_CCW or GLU_CW, then all contours must be of the same type (if they are not, then all GLU_CCW and GLU_CW contours will be changed to GLU_UNKNOWN).

Note that there is no real difference between the GLU_CCW and GLU_CW contour types.

Before the first contour is described, gluNextContour can be called to define the type of the first contour. If gluNextContour is not called before the first contour, then the first contour is marked GLU_EXTERIOR.

This command is obsolete and is provided for backward compatibility only. Calls to gluNextContour are mapped to gluTessEndContour followed by gluTessBeginContour.

## Example

A quadrilateral with a triangular hole in it can be described as follows:

gluBeginPolygon(tobj); gluTessVertex(tobj, v1, v1);
gluTessVertex(tobj, v2, v2);
gluTessVertex(tobj, v3, v3);
gluTessVertex(tobj, v4, v4);
gluNextContour(tobj, GLU_INTERIOR); gluTessVertex(tobj, v5, v5);
gluTessVertex(tobj, v6, v6);
gluTessVertex(tobj, v7, v7);
gluEndPolygon(tobj);

## See Also

gluBeginPolygon(3G) , gluNewTess(3G) , gluTessCallback(3G) , gluTessVertex(3G) , gluTessBeginContour(3G)

Table of Contents

- Name
- C Specification
- Parameters
- Description
- Example
- See Also